|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Door opened | Door closed | Compressor deactivated | Compressor activated |
| Cooler door closed; Idle | Cooler door open; Idle | Cooler door closed; Idle | Cooler door closed; Idle | Cooler door closed; Active |
| Cooler door closed; Active | Cooler door open; Idle | Cooler door closed; Active | Cooler door closed; Idle | Cooler door closed; Active |
| Cooler door open; Idle | Cooler door open; Idle | Cooler door closed; Idle | Cooler door open; Idle | Cooler door open; Idle |